| **DATI TECNICI** | | **ARGO APOLLO 12HP** |
| --- | --- | --- |
| Rated Cooling capacity | kW | 2,35 |
| Energy label class - cooling |  | A |
| Rated Energy Efficiency Ratio |  | 2,61 |
| Hourly energy consumption - cooling | kWh/60 min | 0,9 |
| Rated Heating Capacity | kW | 2,36 |
| Energy label class - heating |  | A |
| Rated COP |  | 3,11 |
| Hourly energy consumption - heating | kWh/60 min | 0,8 |
| Standby mode power consumption | W | 2 |
| Fan speed |  | bassa-media-alta-auto |
| Sound pressure min. | dB(A) | 29 |
| Sound pressure med. | dB(A) | 46 |
| Sound pressure max. | dB(A) | 48 |
| Power supply | V/Ph/Hz | 220-240/1/50 |
| Made in |  | CINA |
| Freon type |  | R32 |
| Freon GWP | KG CO2 EQ. | 675 |
| Freon charge | Kg | 0,39 |
| Freon charge | T CO2 EQ. | 0,26 |
| Max. Dehumidification | l/h | 1 |
| Max. Air flow | m3/h | 480 |
| Available colours |  | bianco |
| Net Height of the unit | mm | 615 |
| Net Width of the unit | mm | 965 |
| Net Depth of the unit | mm | 200 |
| Net Weight of the unit | kg | 36,2 |
| Operation |  | F106 |
| Rated Cooling power input | kW | 0,90 |
| Rated Heating power input | kW | 0,76 |